ErectaStep Distributed by ZeroDocs.com

SECTION 05 51 41 – SAFETY GATES

 GENERAL

 SUBMITTALS

 Action Submittals:

 Product Data: Illustrate products, installation, and relationship to adjacent construction.

 PRODUCTS

 MANUFACTURERS

 Contract Documents are based on products by ErectaStep, [www.erectastep.com](http://www.erectastep.com).

 Substitutions: [Refer to Division 01.] [Not permitted.]

 MATERIALS

 Aluminum:

 Extrusions: ASTM B221.

 Sheet: ASTM B209.

 ACCESSORIES

 Hardware: Corrosion-resistant coated steel.

 FABRICATION

 Safety Gates:

* + - 1. Provide barrier to prevent accidental travel beyond point where gate is installed.
			2. Maximum 108 degree opening.
			3. Self-closing.
			4. Self-stopping.
			5. Field-adjustable tension.
			6. Adjustable swing direction.
			7. Universal mounting.
			8. Width adjustable to fit openings from 16 to 36 inches.
			9. Equip each gate with warning sign.

 FINISHES

 Aluminum: Safety yellow powder coat.

 EXECUTION

 INSTALLATION

 Install in accordance with manufacturer’s instructions.

END OF SECTION