ErectaStep Distributed by ZeroDocs.com

SECTION 05 51 41 – SAFETY GATES

GENERAL

SUBMITTALS

Action Submittals:

Product Data: Illustrate products, installation, and relationship to adjacent construction.

PRODUCTS

MANUFACTURERS

Contract Documents are based on products by ErectaStep, [www.erectastep.com](http://www.erectastep.com).

Substitutions: [Refer to Division 01.] [Not permitted.]

MATERIALS

Aluminum:

Extrusions: ASTM B221.

Sheet: ASTM B209.

ACCESSORIES

Hardware: Corrosion-resistant coated steel.

FABRICATION

Safety Gates:

* + - 1. Provide barrier to prevent accidental travel beyond point where gate is installed.
      2. Maximum 108 degree opening.
      3. Self-closing.
      4. Self-stopping.
      5. Field-adjustable tension.
      6. Adjustable swing direction.
      7. Universal mounting.
      8. Width adjustable to fit openings from 16 to 36 inches.
      9. Equip each gate with warning sign.

FINISHES

Aluminum: Safety yellow powder coat.

EXECUTION

INSTALLATION

Install in accordance with manufacturer’s instructions.

END OF SECTION